|  |  |
| --- | --- |
| **AUGER DOWN REASON CODES** | |
| **REASON** | **CODE** |
| Auger Breakdown | 01 |
| Main Power Loss / Server Down | 02 |
| Truck breakdown at sampling area | 03 |
| Tarpaulin removal not operating | 04 |
| Traffic Jam at truck bay | 05 |
| No Trucks assigned | 06 |
| Preventive maintenance | 07 |
| Lunch Time or Shift change over | 08 |
| Coal cleaning / House keeping | 09 |

Notes:

1. **Code for particular reason to be entered in the HMI screen for auger down status**